1. International AC input range
2. High efficiency,low working temperature
3. Short circuit,overload,over-current protection
4. 100% fully load burn-in test
5. Built-in EMI filter, low ripple noise
6. Low cost, high reliability
7. CE and Rohs approval,2 years warranty
8. OEM and ODM is welcome
	Model
	S-30-5
	

	AC input voltage range
	100-240VAC

	Input current
	0.7A/115V 0.35A/230V

	AC impulse current
	Cold-start current 13A/115V 26A/230V

	DC output voltage
	5V
	

	DC output power
	30W
	

	Rated output current
	6A
	

	Output voltage error 
	±1%
	

	Efficiency
	80%
	

	Wave and noise
	300mVp-p
	

	Inlet stability
	±0.5%
	

	Load stability
	±0.5%
	

	Leakage current
	<0.5mA/240VAC

	Overload protection
	105% - 150% rated power, automatically recovery

	Vibration
	10500Hz,2G 10min./1cycle,Period for 60min,Each axes

	Cooling method
	Natural cooling air convection 

	Working temperature and humidity
	- 20 ° ~ 60 ° c / 20% ~ 90% RH (no frost)

	Store temperature and humidity
	- 40 ° ~ 85 ° c / 10% ~ 95% RH (no frost)

	Safety standards
	CE(EMC+LVD),Rohs

	Dimension
	110x78x35mm

	Weight
	[bookmark: _GoBack]0.21kgs


1.LED switching power supply using pulse width modulation (PWM) switching technology designed to ensure power supply stability and high efficiency. 
2. Product interference, through the EMC testing, ripple ≤ 50MV. 
3. Efficiency above 80%, temperature ≤ 25 °C. 
4.LED switching power supply with overvoltage protection, short circuit protection, overload protection.
5. Constant current output to ensure the stability of the power, so that LED lighting effects better and live longer.
6. Products have the anti-interference ensures long-life LED strips, reducing the LED lighting decline.


